|  |  |
| --- | --- |
| From: ENG Committee |  |
| To: ARM Committee | 21 November 2014 |

Liaison Note to the ANM Committee

NAVGUIDE audible signal update

# Introduction

In liaison note EEP21-14.1.3.13, the EEP Committee proposed amendments to the audible signals section of the NAVGUIDE which remain outstanding.

# Discussion

The present term “sound signals” is now considered to be replaced by “audible signals”. The *Usual Range* table that is Table 2 in Guideline 1090 is technically correct if a note is added that *this only applies to pure (sinusoidal sound)*. It should be noted there are errors in the sound pressure levels in the Nominal Range Table which is Table 1 in Guideline 1090.

# Action Required

The ENG Committee requests that ARM update NAVGUIDE as indicated above.